MESH ANALYTICS
—
SNAPSHOT
Overview
RF / Signal
Traffic
Topology
Health
Environment
Patterns
Links
Node Table
Alerts
Node Score Leaderboard
Bottleneck Nodes
High relay load relative to neighbour redundancy
RF Quality Distribution
Battery Distribution
Node Freshness
Average SNR Over Time
Packet Volume Over Time
Hop Count Distribution
Channel Stress (top 10)
SNR Stability — Most Stable Links
Low SNR variance = consistent RF link quality
Most Unstable RF Links
High SNR std deviation = poor or fluctuating coverage
Daily Message Traffic
Broadcasts
Direct Messages
Daily Active Nodes
Top Broadcasters
Top Relay Nodes
24h vs Prior 24h — Packet Trend per Node
Nodes ranked by activity change
Topology Role Breakdown
Centrality vs RF Health
X: Centrality · Y: RF health · Size: relay count
Isolated & Offline Nodes
Hardware Distribution
Firmware Version Distribution
Resilience Risk Analysis — Single Point of Failure Ranking
Nodes ranked by: route appearances ÷ available neighbours. High risk = mesh heavily depends on this node with few alternatives.
Battery Risk Leaderboard
Combined current level + discharge trend score
Channel Utilisation Risk
Nodes approaching congestion thresholds
Node Score Distribution
Distribution of composite health scores across all nodes
No environmental sensor data found. Nodes with BME280/BME680 sensors will show data here.
Sensor Nodes — Current Readings
Temperature Over Time
Humidity Over Time
Hourly Activity Heatmap — Packets by Hour of Day (last 7 days)
Identifies peak activity windows and quiet hours
Low
High
Daily RF + Traffic Combined View
Avg SNR (dB)
RF Packets (÷10)
Messages
Most Active Nodes — Last 24h vs Prior 24h
Last 24h
Prior 24h
Most-Used Route Links
Ranked by number of traceroute appearances — these are the critical links in your mesh backbone
Neighbour SNR Matrix
All known neighbour pairs with SNR readings
Link Usage vs SNR Quality
X: usage count · Y: avg SNR of endpoints

Detected Conditions