WEB TELEMETRY
[ SELECT A DESTINATION NODE FROM THE SIDEBAR ]
Phase 1: Target Acquisition
Phase 2: Payload Extraction
PAGE 1
Phase 3: RF Transmission
PAYLOAD: None
DESTINATION: None
Sensor Label (Prefix)
Mesh Channel
Manual transmission:
Automated Cron Directive
Schedule
Time / Date
CRONTAB: * * * * *

#### WEB-TO-RF BRIDGE

Extract data from websites and broadcast over the mesh network.

##### 1. Acquisition

Enter a public URL. The backend parses the DOM into text blocks.

##### 2. Extraction

Select the text block to monitor.

##### 3. Deployment

Transmit immediately or schedule a cron task.

##### Use Cases

• Weather data
• Server status
• Stock prices
• Any public web data