NETWORK INTELLIGENCE
LINK QUALITY · SMART HOPS · ENTROPY · RELAY ANALYSIS
MESH ENTROPY —
FLEET HEALTH
—
LOADING
Updated —
—
TOTAL NODES
—
ACTIVE / 1H
—
SILENT >3H
—
AVG SNR dB
—
CH UTIL %
—
AVG BATTERY
PACKET RATE — 24H
24H AGO NOW
LQS DISTRIBUTION
FLEET AVG SNR TREND
TOP TALKERS — 24H
ROLE DISTRIBUTION
SELECT A NODE FROM THE LIST FOR DETAILED LINK QUALITY ANALYSIS
LINK QUALITY SCORE
—
OUT OF 10
—
SNR dB
—
AVG HOP
—
HOP σ
SCORE COMPONENTS
SCORING FORMULA
Base 5.0 · +1.0 SNR>-5dB · +0.5 SNR>-10dB · -0.5 SNR>-15dB · -1.5 SNR<-15dB
+0.5 stable routing · -1.0 route flapping · +1.0 traceroute ok · -2.0 traceroute failed
-5.0 PKI error · -1.0 silent >3× interval · +0.5 direct neighbor confirmed · Clamped 0–10
SMART HOPS — 24H WINDOW 15-minute buckets · hopStart − hopLimit
HOP VARIANCE ANALYSIS
SNR / RSSI HISTORY
RSSI HISTORY
FLEET HEALTH SUMMARY
CRITICAL NODES (LQS < 4)
LQS DISTRIBUTION
RELAY CONTRIBUTION 24h traffic load · larger = more relay activity
WHAT THIS MEANS
Nodes with high relay load are critical infrastructure — if they fail, large parts of the mesh lose connectivity.
High load + ROUTER role = expected. High load + CLIENT role = potential misconfiguration.
Relay concentration (Gini) above 0.7 means your mesh depends heavily on 1–2 nodes.
TRACEROUTE HISTORY
DIRECT RF NEIGHBORS Nodes that reported this node as 1-hop neighbor