NODE MONITOR
ACTIVE
New Monitor Rule
[ SELECT A NODE FROM THE SIDEBAR TO CONFIGURE ]
TARGET:
Metric
Condition
Threshold
Alert Type
Broadcast to Channel Direct to Node
Broadcast Channel
Destination Node
Via Channel
Check Frequency (mins)
Send Alert Via Radio
Active Monitor Rules

Target | Condition | Destination | Frequency | Via Radio | Actions
--- | --- | --- | --- | --- | ---
[ NO RULES CONFIGURED ]