CHANNEL VAULT
SERVER-SIDE PSK DECRYPTION · UNLIMITED CHANNELS · HOTSWAP · BACKUP & RESTORE
ADD CHANNEL PSK
CHANNEL NAME
PSK (base64)
1 byte ("AQ=="), 16 bytes (AES-128), or 32 bytes (AES-256)
NOTES (optional)
PRIORITY
SLOT HINT
Uplink enabled
Downlink enabled
RADIO SLOT (for retroactive decrypt)
ENCRYPTED PACKETS FROM UNKNOWN CHANNELS — click to add PSK or hotswap
SERVER-SIDE DECRYPTED PACKETS — packets the radio couldn't decode
SNAPSHOT RADIO CHANNELS

Read all 8 channel slots from the connected radio and save them to the vault database. Includes channel names, PSKs, and settings. Use before hotswapping to preserve the current state.

RADIO SLOT
LABEL (optional)
HOW BACKUP WORKS
① SNAPSHOT — reads current radio channels into vault DB.
② IMPORT TO VAULT — copies channel PSKs from backup into the server-side decryption vault.
③ HOTSWAP — writes any vaulted channel to a specific radio slot, then optionally reboots.
④ RESTORE — hotswap each backup channel back to its original slot to undo changes.
SAVED BACKUPS
Channel Hotswap
Write any vaulted channel directly to one of the radio's 8 slots and reboot. The radio must reboot for the new channel config to take effect on the mesh. Always snapshot first so you can restore if needed.
SELECT VAULT CHANNEL
SELECT RADIO SLOT
Current radio channel map — click a slot to target it
OPTIONS
ROLE
REBOOT DELAY (seconds)
Reboot radio after write
Uplink enabled
Downlink enabled