● Active—
◑ Recent—
◔ Aging—
○ Floor—
Total—
Mesh Health—
MeshDash
Tactical Network Monitor
Connection—
Local Node—
Mesh Status—
—
● <30m — Active
◑ 30m–1h — Recent
◔ 1h–24h — Aging
○ 24h–72h — Floor
Stale >48h
Packet Feed
▶ Stream
X: 0.0 Y: 0.0 Z: —
Node
Direct Message
Reply to —
Live
—
—
—
● Active ★ Local — —
—
Hardware
Model
—
Firmware
—
MAC
—
Node Num
—
Signal Quality
SNR
— dB
RSSI
— dBm
Hops
—
Channel
—
Power
Battery
— %
Voltage
— V
Ch Util
— %
Air Util TX
— %
Uptime
—
Session Pkts
—
GPS Position
Coordinates
—
Altitude
— m
Precision
—
Speed
—
Sats
—
Fix Time
—
Database Counts
Messages Sent
—
Position Records
—
Telemetry Records
—
Telemetry Time
—
⚠ NODE OFFLINE
Battery History (last 14)
Environment Sensors
Temperature
— °C
Humidity
— %
Pressure
— hPa
Gas / IAQ
—
Telemetry Log (last 10)
Loading…
Ping Estimate
Latency—
Neighbours
Loading…
Traceroutes
Loading…
Position Track (last 8)
Loading…
Message History
Loading…