Skip to content
C2 COMMAND TERMINAL
Init...
!AWAITING
Loading...
ONLINE ACCESS: FULL
UPTIME / STABILITY TREND

### System Dialog

### SYSTEM DIAGNOSTICS

Real-time local node status · RF config · hardware telemetry

Dashboard
-
Tab / SSE Session
SSE stream open time
Process
-
Python Backend Runtime
since process start
Firmware
-
Radio Node Uptime
since last firmware boot
IDENTITY
Node ID-
Short Name-
Long Name-
Hardware-
Firmware-
Role-
Reboots-
RF / LORA
Region-
LoRa Region-
Hop Limit-
TX Power-
TX State-
NodeDB-
Ch Util-
POWER & NETWORK
Battery-
Voltage-
Battery Level
Air Util TX-
Bluetooth-
Position-
Altitude-
CONNECTION HEALTH (24H)
API Stream
Connecting…
Radio Link
Initializing
Radio Link History (24h)
LIVE TRAFFIC MONITOR
[ AWAITING TRAFFIC ]
ℹ️ Notification
Initialising Vitals...
meshtastic >
CONFIRM UPDATE (Y/N) >